# Technical Data

Ordering No | 8411101168
Model | LZL15-L-P-IEC
Air consumption at 3000 RPM | l/s
Air consumption at 3000 RPM | cfm
Air consumption at max output | 61 l/s
Air consumption at max output | 129 cfm
External parts material | Powder coated cast iron
Free speed | 7000 r/min
Inlet hose | 25 mm
Inlet hose | 1 in
Max allowed speed | r/min
Max ambient temperature | 40 ºC
Max output | 2.3 kW
Max output | 3.1 hp
Max radial load at max output | N
Min starting torque | 10.9 Nm
Min starting torque | 8 ft lb
Mounting arrangement |
Outlet hose | 25 mm
Outlet hose | 1 in
Power at 3000 RPM | kW
Power at 3000 RPM | hp
Ratio |
Rotation direction | Reversible
Shaft loading code |
Speed at max output | 3380 r/min
Stall torque | 13 Nm
Stall torque | 9.6 ft lb
Torque at max output | 6.5 Nm
Torque at max output | 4.8 ft lb
Vane type | Lubrication free
Weight | 8.3 kg
Weight | 18.3 lb