# Tightening

WARNING

Risk of Injury

Make sure that the correct parameter file is being used. Wrong parameter file might cause too high torque with bodily injury as a result.

- Compare the maximum torque which is shown in the controller, with the maximum torque stated in the technical data of the tool, they should be the same.

## Rotation Direction for the Tightening

Check that the tool is in the correct running direction by turning the reverse button or reverse ring.

Pistol Grip Models (with side buttons)

- Press the reverse switch on the right hand side of the tool, to set the direction clockwise (CW).

- Press the reverse switch on the left hand side of the tool, to set the direction counter-clockwise (CCW).

Pistol Grip Models (without side buttons)

- Double press the function button on the top of the start trigger to shift the direction between clockwise (CW) and counter-clockwise (CCW).

Angle Models

- Turn the reverse ring to the right, to set the direction clockwise (CW).

- Turn the reverse ring to the left, to set the direction counter-clockwise (CCW).

## Soft Start

The soft start function facilitates the screw head and thread to reach the snug level. The duration of the soft start is adjustable.

For further information about tightening, see Power Focus 6000 Configuration manual.