# Torque Check on Actual Joint

1. Use the same equipment and settings. For example extensions, sockets and tightening program on the test joint, as will be used on the actual joint.

2. When performing a torque check on the actual joint we recommend using an STWrench with residual measurement* setting.

* Torque required to cause the threads of the fastener (including its head) on which torque is applied, to move relative to the mating thread.

A | The actual joint
B | Torque wrench

1. Perform a tightening.

2. Measure the result with the Torque wrench.

3. If the residual torque is not according to the target torque, adjust tightening parameters.