# LED Indicator (HMI)

Indicator position | LED indicator | Main indication
--- | --- | ---
1 | Green | Tightening result OK
2 | Red | Tightening result NOK
3 | Yellow | Tightening result warning
4 | White | Tightening direction
5 | Green | Batch OK complete
6 | Battery | Battery charge status
7 | Blue | Radio connection established with POWER FOCUS 6000/ToolsTalk Service 2
8 | Blue | Configurable - can be configured in the controller to indicate different events
9 | Red | Alarm error has occurred in the tool

For more information, see LED Indicator Flash Patterns.