# Tool Condition Test

A | Static Torque Transducer SRTT
B | STa6000

## Test the maximum torque and pulse frequency

Set the filter frequency in STa6000 to 850 Hz.

Test the max torque and pulse frequency using a SRTT static torque transducer. Tightening time approximately 1 second.

## Test Conditions

Temperature pulse unit: approximately 20° C.

In POWER FOCUS 6000, change Tool → Adjustment → Torque Adjustment Factor to 50%, prevents the tool from shutting off. Measure torque and pulse frequency rate clockwise in the SRTT for about 1 second. Check that the values meet the specified limits in table below.

A tool in good condition should achieve the following values:

Model | Pulse frequency | Max Torque CW static (minimum) (Nm)
--- | --- | ---
ETP TBP/TBP-S 6 | 12-20 Hz | > 42 Nm
ETP TBP/TBP-S 6 (42) | 10-18 Hz | >39 Nm
ETP TBP/TBP-S 8 | 11-20 Hz | > 64 Nm
ETP TBP/TBP-S 9 | 10-19 Hz | > 97 Nm
ETP TBP/TBP-S 13 | 8-15 Hz | > 181 Nm