# MWR Charging cradle

To recharge the battery of the MWR-200 TA with the MWR Charging Cradle:

1. Connect the MWR Charging Cradle to the AC power.

2. Insert the MWR-200 TA into the MWR Charging Cradle:

   When the wrench is placed into the MWR Charging Cradle, the red, yellow and green LEDs (placed on three sides of the MWR-200 TA) flash alternately. This indicates that the wrench sets the internal offset (zero point) for the torque transducer and runs a quick self-test.

   When the MWR-200 TA is in charging mode and the internal offset has been performed, the yellow LED of the MWR-200 TA is on and the Status LED of the MWR Charging Cradle is flashing (green colored).

   When the charging process of the MWR-200 TA is complete, the Status LED of the MWR Charging Cradle is constantly on (green colored).

For more information on the MWR Charging Cradle functioning, refer to the MWR Charging Cradle Product Instructions.