# Guide

Ordering No. | Thread | Remark
--- | --- | ---
4141 0883 91 | M6x1 | Max stroke 55 mm. Suitable for concentric collet MINI and REGULAR.
4141 0883 90 | M6x1 | Max stroke 25 mm. Suitable for concentric collet MINI and REGULAR.
4141 0883 94 | M8x1 | Max stroke 55 mm. Suitable for concentric collet MINI and REGULAR.
4141 0883 93 | M8x1 | Max stroke 25 mm. Suitable for concentric collet MINI and REGULAR.
4141 0883 95 | M8x1 | Max stroke 40 mm. Suitable for concentric collet HD.
4141 0883 97 | M10x1 | Max stroke 40 mm. Suitable for concentric collet HD.
4141 0883 96 | M8x1 | Max stroke 62 mm. Suitable for concentric collet HD.
4141 0883 98 | M10x1 | Max stroke 62 mm. Suitable for concentric collet HD.