# Guide Bushing

Ordering No. | Remark
--- | ---
4141 0707 90 | Max stroke 44 mm, spacer length 22 mm. Suitable for concentric collet MINI and REGULAR.
4141 0707 92 | Max stroke 52 mm, spacer length 30 mm. Suitable for concentric collet MINI and REGULAR.
4141 0707 94 | Max stroke 62 mm, spacer length 40 mm. Suitable for concentric collet MINI and REGULAR.
4141 0707 96 | Max stroke 73 mm, spacer length 50 mm. Suitable for concentric collet MINI and REGULAR.
4141 0868 90 | Max stroke 25 mm, spacer length 22 mm. Suitable for concentric collet MINI and REGULAR.
4141 0868 91 | Max stroke 55 mm, spacer length 50 mm. Suitable for concentric collet MINI and REGULAR.
4141 0868 94 | Max stroke 40 mm, spacer length 50 mm. Suitable for concentric collet HD.
4141 0868 95 | Max stroke 62 mm, spacer length 50 mm. Suitable for concentric collet HD.
4141 0868 96 | Max stroke 65 mm, spacer length 95 mm. Suitable for concentric collet MINI and REGULAR.
4141 0894 90 | Max stroke 65 mm, spacer length 26 mm. Suitable for concentric collet HD.
4141 0894 92 | Max stroke 75 mm, spacer length 35 mm. Suitable for concentric collet HD.
4141 0894 94 | Max stroke 85 mm, spacer length 45 mm. Suitable for concentric collet HD.
4141 0894 96 | Max stroke 95 mm, spacer length 55 mm. Suitable for concentric collet HD.