# Required Accessories

# Feed Cassette

Ordering No. | IPR | mm/rev
--- | --- | ---
4141 0428 91 | 0.0011 alt. 0.0064 | 0.028 alt. 0.16
4141 0428 93 | 0.0028 alt. 0.0045 | 0.071 alt. 0.12
4141 0428 94 | 0.0037 | 0.093
4141 0428 95 | 0.0007 alt. 0.0068 | 0.017 alt. 0.17
4141 0428 96 | 0.0015 alt. 0.0059 | 0.038 alt. 0.15
4141 0428 97 | 0.0021 alt. 0.0052 | 0.054 alt. 0.13

# Spindle

Ordering No. | Length | Thread (UNF)
--- | --- | ---
4141 0404 90 | 135 mm (5.3") | 3/8"
4141 0404 91 | 160 mm (6.3") | 3/8"
4141 0404 92 | 185 mm (7.3") | 3/8"
4141 0404 93 | 236 mm (9.3") | 3/8"
4141 0404 94 | 210 mm (8.3") | 3/8"
4141 0404 95 | 287 mm (11.3") | 3/8"
4141 0651 90 | 135 mm (5.3") | 1/4"
4141 0651 91 | 160 mm (6.3") | 1/4"
4141 0651 92 | 185 mm (7.3") | 1/4"
4141 0651 93 | 210 mm (8.3") | 1/4"
4141 0651 94 | 236 mm (9.3") | 1/4"
4141 0652 90 | 135 mm (5.3") | 5/16"
4141 0652 91 | 160 mm (6.3") | 5/16"
4141 0652 92 | 185 mm (7.3") | 5/16"
4141 0652 93 | 210 mm (8.3") | 5/16"
4141 0652 94 | 236 mm (9.3") | 5/16"
4141 0653 90 | 194 mm (7.6") | 9/16"
4141 0653 91 | 245 mm (9.7") | 9/16"
4141 0653 92 | 219 mm (8.6") | 9/16"
4141 0653 93 | 296 mm (11.7”) | 9/16"
4141 0869 94 | 245 mm (9") | 7/16"

# Spindle Guard

Ordering No. | Suitable for spindles
--- | ---
4141 0472 90 | 4141 0404 92, 4141 0651 92, 4141 0652 92, 4141 0653 92
4141 0472 91 | 4141 0404 90, 4141 0651 90, 4141 0652 90
4141 0472 92 | 4141 0404 91, 4141 0651 91, 4141 0652 91
4141 0472 93 | 4141 0404 93, 4141 0651 94, 4141 0652 94, 4141 0653 91
4141 0472 94 | 4141 0404 92, 4141 0651 92, 4141 0652 92, 4141 0653 92
4141 0472 95 | 4141 0404 90, 4141 0651 90, 4141 0652 90
4141 0472 96 | 4141 0404 91, 4141 0651 91, 4141 0652 91
4141 0472 97 | 4141 0404 93, 4141 0651 94, 4141 0652 94, 4141 0653 91
4141 0472 98 | 4141 0404 94, 4141 0651 93, 4141 0652 93, 4141 0653 92
4141 0472 99 | 4141 0404 94, 4141 0651 93, 4141 0652 93, 4141 0653 92
4141 0829 90 | 4141 0404 95, 4141 0653 93
4141 0829 91 | 4141 0404 95, 4141 0653 93

# Spindle Guard Coolant

For angle models
Ordering No. | Suitable for spindles
--- | ---
4141 0826 90 | 4141 0404 92, 4141 0651 92, 4141 0652 92, 4141 0653 92
4141 0826 91 | 4141 0404 91, 4141 0651 91, 4141 0652 91
4141 0826 92 | 4141 0404 90, 4141 0651 90, 4141 0652 90
4141 0826 93 | 4141 0404 94, 4141 0651 93, 4141 0652 93, 4141 0653 92
4141 0826 94 | 4141 0404 93, 4141 0651 94, 4141 0652 94, 4141 0653 91
4141 0826 95 | 4141 0404 95, 4141 0653 93

For in-line models
Ordering No. | Suitable for spindles
--- | ---
4141 0878 90 | Suitable for all spindles.

# Optional Accessories

# Adapter

Ordering No. | Interface
--- | ---
4141 0032 04 | 1 9/16"-20 UN 2B L.H internal threads
4141 0032 07 | 1.825-18 NS L.H external threads
4141 0274 90 | 1"-20 UNEF 2A L.H external threads

# Front Part

Ordering No. | Length | Thread | Remark
--- | --- | --- | ---
4141 0654 94 | 75 mm (3.0") | 3/4"-16 UNF | Cannot be used with Scraper nut
4141 0654 96 | 75 mm (3.0") | 3/4"-16 UNF | Cannot be used with Scraper nut
4141 0886 94 | 75 mm (3.0") | 3/4"-16 UNF | Can be used with Scraper nut 4141 0884 90.
4141 0886 96 | 75 mm (3.0") | 3/4"-16 UNF | Can be used with Scraper nut 4141 0884 90.
4141 0654 93 | 90 mm (3.5") | 3/4"-16 UNF | Cannot be used with Scraper nut
4141 0886 93 | 90 mm (3.5") | 3/4"-16 UNF | Can be used with Scraper nut 4141 0884 90.
4141 0654 90 | 127 mm (5") | 3/4"-16 UNF | Cannot be used with Scraper nut
4141 0886 90 | 127 mm (5") | 3/4"-16 UNF | Can be used with Scraper nut 4141 0884 90.
4141 0261 94 | 75 mm (3.0") | 1"-14 UNF | Cannot be used with Scraper nut
4141 0261 98 | 75 mm (3.0") | 1"-14 UNF | Cannot be used with Scraper nut
4141 0261 93 | 90 mm (3.5") | 1"-14 UNF | Cannot be used with Scraper nut
4141 0261 90 | 127 mm (5") | 1"-14 UNF | Cannot be used with Scraper nut
4141 0887 90 | 127 mm (5") | 1"-14 UNF | Can be used with Scraper nut 4141 0884 90.
4141 0261 91 | 203 mm (8") | 1"-14 UNF | Cannot be used with Scraper nut
4141 0887 91 | 203 mm (8") | 1"-14 UNF | Can be used with Scraper nut 4141 0884 90.
4141 0261 92 | 305 mm (12") | 1"-14 UNF | Cannot be used with Scraper nut
4141 0887 92 | 305 mm (12") | 1"-14 UNF | Can be used with Scraper nut 4141 0884 90.
4141 0251 90 | 127 mm (5") | 1 1/4"-12 UNF | Can be used with Scraper nut 4141 0884 90. Requires Scraper Tube 4141 0885 00
4141 0251 91 | 203 mm (8") | 1 1/4"-12 UNF | Can be used with Scraper nut 4141 0884 90. Requires Scraper Tube 4141 0885 00
4141 0251 92 | 305 mm (12") | 1 1/4"-12 UNF | Can be used with Scraper nut 4141 0884 90. Requires Scraper Tube 4141 0885 00
4141 0245 92 | 127 mm (5") | 1 1/2"-12 UNF | Can be used with Scraper nut 4141 0884 90. Requires Scraper Tube 4141 0885 00
4141 0245 90 | 200 mm (8") | 1 1/2"-12 UNF | Can be used with Scraper nut 4141 0884 90. Requires Scraper Tube 4141 0885 00
4141 0245 94 | 200 mm (8") | 1 1/2"-12 UNF | Can be used with Scraper nut 4141 0884 90. Requires Scraper Tube 4141 0885 00
4141 0245 91 | 300 mm (12") | 1 1/2"-12 UNF | Can be used with Scraper nut 4141 0884 90. Requires Scraper Tube 4141 0885 00
4141 0257 90 | 203 mm (8”) | 2”-16 UNF | Can be used with Scraper nut 4141 0884 90.
4141 0257 91 | 305 mm (12”) | 2”-16 UNF | Can be used with Scraper nut 4141 0884 90.
4141 0899 92 | 90 mm (3.5") | 1"- 14 UNF | Can only be used with swiveling vacuum attachments.
4141 0899 93 | 90 mm (3.5") | 1 1/4"-12 UNF | Can only be used with swiveling vacuum attachments.

# Extension

Ordering No. | Length | Thread | Remarks
--- | --- | --- | ---
4141 0901 00 | 51 mm (1.5") | 1"-20 UNF | Compatible with standard indexer and front part 4141 0899 92.
4141 0902 00 | 52 mm (1.5") | 1 9/16"-20 UNF | Must be used with HD indexer and front part 4141 0899 93.
4141 0902 01 | 77 mm (2.5") | 1 9/16"-20 UNF | Must be used with HD indexer and front part 4141 0899 93.
4141 0902 02 | 103 mm (3.5") | 1 9/16"-20 UNF | Must be used with HD indexer and front part 4141 0899 93.

# Vacuum Attachment

Ordering No. | Suitable for front part
--- | ---
4141 0250 91 | 4141 0261 90
4141 0250 92 | 4141 0261 91
4141 0250 93 | 4141 0251 90
4141 0250 94 | 4141 0261 92
4141 0250 95 | 4141 0251 91
4141 0250 96 | 4141 0251 92
4141 0250 97 | 4141 0245 91
4141 0250 98 | 4141 0257 90
4141 0250 99 | 4141 0257 91
4141 0330 90 | 4141 0245 92
4141 0250 90 | 4141 0245 90
4141 0900 92 | Suitable for all swiveling front part (4141 090X XX)

# ChipLet

Ordering No. | Remark
--- | ---
4141 0509 91 | 0 rollers, 0 amplitude
4141 0713 91 | 3 rollers, 0.10 amplitude
4141 0713 92 | 3 rollers, 0.15 amplitude
4141 0713 93 | 3 rollers, 0.20 amplitude
4141 0713 94 | 3 rollers, 0.25 amplitude
4141 0759 91 | 5 rollers, 0.10 amplitude
4141 0759 92 | 5 rollers, 0.15 amplitude
4141 0759 93 | 5 rollers, 0.20 amplitude
4141 0759 94 | 5 rollers, 0.25 amplitude
4141 0759 95 | 5 rollers, 0.05 amplitude

# Concentric Collet

Ordering No. | Total weight | Remark
--- | --- | ---
4141 0764 90 | 0.5 kg | MINI
4141 0670 92 | 0.75 kg | REGULAR
4141 0702 91 | 1.0 kg | HD

# Mandrel

Ordering No. | Type | Remark
--- | --- | ---
4141 0806 05 | A | Ød 9.2 mm. Order together with 4141 0813 05. Suitable for concentric collet MINI and REGULAR.
4141 0806 08 | A | Ød 10.2 mm. Order together with 4141 0813 08. Suitable for concentric collet MINI and REGULAR.
4141 0806 09 | A | Ød 10.5 mm. Order together with 4141 0813 09. Suitable for concentric collet MINI and REGULAR.
4141 0806 10 | A | Ød 10.9 mm. Order together with 4141 0813 10. Suitable for concentric collet MINI and REGULAR.
4141 0806 11 | A | Ød 11.25 mm. Order together with 4141 0813 11. Suitable for concentric collet MINI and REGULAR.
4141 0806 12 | A | Ød 11.5 mm. Order together with 4141 0813 12. Suitable for concentric collet MINI and REGULAR.
4141 0806 13 | A | Ød 11.9 mm. Order together with 4141 0813 13. Suitable for concentric collet MINI and REGULAR.
4141 0806 14 | A | Ød 12.3 mm. Order together with 4141 0813 14. Suitable for concentric collet MINI and REGULAR.
4141 0806 15 | A | Ød 12.7 mm. Order together with 4141 0813 15. Suitable for concentric collet MINI and REGULAR.
4141 0806 16 | A | Ød 20.6 mm. Order together with 4141 0813 16. Suitable for concentric collet MINI and REGULAR.
4141 0806 18 | A | Ød 13.9 mm. Order together with 4141 0813 18. Suitable for concentric collet MINI and REGULAR.
4141 0806 20 | A | Ød 14.7 mm. Order together with 4141 0813 20. Suitable for concentric collet MINI and REGULAR.
4141 0806 21 | A | Ød 15.1 mm. Order together with 4141 0813 21. Suitable for concentric collet MINI and REGULAR.
4141 0806 22 | A | Ød 15.5 mm. Order together with 4141 0813 22. Suitable for concentric collet MINI and REGULAR.
4141 0806 23 | A | Ød 15.9 mm. Order together with 4141 0813 23. Suitable for concentric collet MINI and REGULAR.
4141 0806 24 | A | Ød 16.3 mm. Order together with 4141 0813 24. Suitable for concentric collet MINI and REGULAR.
4141 0806 26 | A | Ød 17.1 mm. Order together with 4141 0813 26. Suitable for concentric collet MINI and REGULAR.
4141 0806 28 | A | Ød 17.9 mm. Order together with 4141 0813 28. Suitable for concentric collet MINI and REGULAR.
4141 0860 03 | A | Ød 4.14 mm. Order together with 4141 0813 03. Suitable for concentric collet MINI and REGULAR.
4141 0809 09 | A | Ød 21.5 mm. Order together with 4141 0814 09. Suitable for concentric collet HD.
4141 0809 10 | A | Ød 29.4 mm. Order together with 4141 0814 10. Suitable for concentric collet HD.
4141 0809 11 | A | Ød 29.8 mm. Order together with 4141 0814 11. Suitable for concentric collet HD.
4141 0809 16 | A | Ød 31.75 mm (1 1/4" mm). Order together with 4141 0814 16. Suitable for concentric collet HD.
4141 0809 17 | A | Ød 24.6 mm. Order together with 4141 0814 17. Suitable for concentric collet HD.
4141 0676 01 | B | Ød 5 mm. Order together with 4141 0813 01. Suitable for concentric collet MINI and REGULAR.
4141 0676 02 | B | Ød 6.7 mm. Order together with 4141 0813 02. Suitable for concentric collet MINI and REGULAR.
4141 0676 03 | B | Ød 14.7 mm. Order together with 4141 0813 20. Suitable for concentric collet MINI and REGULAR.
4141 0676 04 | B | Ød 17.9 mm. Order together with 4141 0813 28. Suitable for concentric collet MINI and REGULAR.
4141 0676 05 | B | Ød 11.5 mm. Order together with 4141 0813 12. Suitable for concentric collet MINI and REGULAR.
4141 0676 06 | B | Ød 7.5 mm. Order together with 4141 0813 03. Suitable for concentric collet MINI and REGULAR:
4141 0810 03 | B | Ød 21.75 mm. Order together with 4141 0814 08. Suitable for concentric collet HD.
4141 0810 04 | B | Ød 24.25 mm. Order together with 4141 0814 16. Suitable for concentric collet HD.
4141 0810 05 | B | Ød 26.65 mm. Order together with 4141 0814 24. Suitable for concentric collet HD.
4141 0807 01 | C | Ød 5 mm. Order together with 4141 0813 01. Suitable forconcentric collet MINI and REGULAR.
4141 0807 03 | C | Ød 7.6 mm. Order together with 4141 0813 03. Suitable for concentric collet MINI and REGULAR.

# Collet

Ordering No. | Remark
--- | ---
4141 0677 03 | ØD 22.9 mm. Order together with 4141 0676 03.
4141 0677 04 | ØD 25.2 mm. Order together with 4141 0676 04.
4141 0814 08 | ØD 28.58 mm (1 1/8"). Order together with 4141 0810 03. Suitable for concentric collet HD.
4141 0814 16 | ØD 31.75 mm (1 1/4"). Order together with 4141 0810 04. Suitable for concentric collet HD.
4141 0814 24 | ØD 34.93 mm (1 3/8"). Order together with 4141 0810 05. Suitable for concentric collet HD.
4141 0813 01 | ØD 12.7 mm. Order together with 4141 0806 01 or 4141 0807 01 or 4141 0676 01. Suitable for concentric collet MINI and REGULAR.
4141 0813 02 | ØD 15.09 mm. Order together with 4141 0676 02. Suitable for concentric collet MINI and REGULAR.
4141 0813 03 | ØD 15.87 mm (5/8"). Order together with 4141 0806 03 or 4141 0807 03 or 4141 0676 06 or 4141 0860 03. Suitable for concentric collet MINI and REGULAR.
4141 0813 05 | ØD 16.7 mm. Order together with 4141 0806 05. Suitable for concentric collet MINI and REGULAR.
4141 0813 06 | ØD 17 mm. Order together with 4141 0806 05. Suitable for concentric collet MINI and REGULAR.
4141 0813 08 | ØD 17.7 mm. Order together with 4141 0806 08. Suitable for concentric collet MINI and REGULAR.
4141 0813 09 | ØD 18.05 mm. Order together with 4141 0806 09. Suitable for concentric collet MINI and REGULAR.
4141 0813 10 | ØD 18.4 mm. Order together with 4141 0806 10. Suitable for concentric collet MINI and REGULAR.
4141 0813 11 | ØD 18.75 mm. Order together with 4141 0806 11. Suitable for concentric collet MINI and REGULAR.
4141 0813 12 | ØD 19.05 mm (3/4"). Order together with 4141 0806 12. Suitable for concentric collet MINI and REGULAR.
4141 0813 13 | ØD 19.4 mm. Order together with 4141 0806 13. Suitable for concentric collet MINI and REGULAR.
4141 0813 14 | ØD 19.8 mm. Order together with 4141 0806 14. Suitable for concentric collet MINI and REGULAR.
4141 0813 15 | ØD 20.2 mm. Order together with 4141 0806 15. Suitable for concentric collet MINI and REGULAR.
4141 0813 16 | ØD 20.6 mm. Order together with 4141 0806 16. Suitable for concentric collet MINI and REGULAR.
4141 0813 18 | ØD 21.4 mm. Order together with 4141 0806 18. Suitable for concentric collet MINI and REGULAR.
4141 0813 20 | ØD 22.22 mm (7/8"). Order together with 4141 0806 20. Suitable for concentric collet MINI and REGULAR.
4141 0813 21 | ØD 22.6 mm. Order together with 4141 0806 21. Suitable for concentric collet MINI and REGULAR.
4141 0813 22 | ØD 23 mm. Order together with 4141 0806 22. Suitable for concentric collet MINI and REGULAR.
4141 0813 23 | ØD 23.4 mm. Order together with 4141 0806 23. Suitable for concentric collet MINI and REGULAR.
4141 0813 24 | ØD 23.8 mm. Order together with 4141 0806 24. Suitable for concentric collet MINI and REGULAR.
4141 0813 26 | ØD 24.6 mm. Order together with 4141 0806 26. Suitable for concentric collet MINI and REGULAR.
4141 0813 28 | ØD 25.4 mm (1"). Order together with 4141 0806 28. Suitable for concentric collet MINI and REGULAR.
4141 0813 29 | ØD 26 mm. Order together with 4141 0806 28 or 4141 0807 28 or 4141 0676 04. Suitable for concentric collet MINI and REGULAR.
4141 0814 08 | ØD 28.58 mm. Order together with 4141 0810 03. Suitable for concentric collet HD.
4141 0814 09 | ØD 29 mm. Order together with 4141 0809 09. Suitable for concentric collet HD.
4141 0814 10 | ØD 29.4 mm. Order together with 4141 0809 10. Suitable for concentric collet HD.
4141 0814 11 | ØD 29.8 mm. Order together with 4141 0809 11. Suitable for concentric collet HD.
4141 0814 16 | ØD 31.75 mm (1 1/4"). Order together with 4141 0810 04. Suitable for concentric collet HD.
4141 0814 17 | ØD 32.15 mm. Order together with 4141 0809 17. Suitable for concentric collet HD.
4141 0814 24 | ØD 34.93 mm. Order together with 4141 0810 05. Suitable for concentric collet HD.

# Guide

Ordering No. | Thread | Remark
--- | --- | ---
4141 0883 91 | M6x1 | Max stroke 55 mm. Suitable for concentric collet MINI and REGULAR.
4141 0883 90 | M6x1 | Max stroke 25 mm. Suitable for concentric collet MINI and REGULAR.
4141 0883 94 | M8x1 | Max stroke 55 mm. Suitable for concentric collet MINI and REGULAR.
4141 0883 93 | M8x1 | Max stroke 25 mm. Suitable for concentric collet MINI and REGULAR.
4141 0883 95 | M8x1 | Max stroke 40 mm. Suitable for concentric collet HD.
4141 0883 97 | M10x1 | Max stroke 40 mm. Suitable for concentric collet HD.
4141 0883 96 | M8x1 | Max stroke 62 mm. Suitable for concentric collet HD.
4141 0883 98 | M10x1 | Max stroke 62 mm. Suitable for concentric collet HD.

# Guide Bushing

Ordering No. | Remark
--- | ---
4141 0707 90 | Max stroke 44 mm, spacer length 22 mm. Suitable for concentric collet MINI and REGULAR.
4141 0707 92 | Max stroke 52 mm, spacer length 30 mm. Suitable for concentric collet MINI and REGULAR.
4141 0707 94 | Max stroke 62 mm, spacer length 40 mm. Suitable for concentric collet MINI and REGULAR.
4141 0707 96 | Max stroke 73 mm, spacer length 50 mm. Suitable for concentric collet MINI and REGULAR.
4141 0868 90 | Max stroke 25 mm, spacer length 22 mm. Suitable for concentric collet MINI and REGULAR.
4141 0868 91 | Max stroke 55 mm, spacer length 50 mm. Suitable for concentric collet MINI and REGULAR.
4141 0868 94 | Max stroke 40 mm, spacer length 50 mm. Suitable for concentric collet HD.
4141 0868 95 | Max stroke 62 mm, spacer length 50 mm. Suitable for concentric collet HD.
4141 0868 96 | Max stroke 65 mm, spacer length 95 mm. Suitable for concentric collet MINI and REGULAR.
4141 0894 90 | Max stroke 65 mm, spacer length 26 mm. Suitable for concentric collet HD.
4141 0894 92 | Max stroke 75 mm, spacer length 35 mm. Suitable for concentric collet HD.
4141 0894 94 | Max stroke 85 mm, spacer length 45 mm. Suitable for concentric collet HD.
4141 0894 96 | Max stroke 95 mm, spacer length 55 mm. Suitable for concentric collet HD.

# Other Accessories

Accessory | Ordering No.
--- | ---
Display counter | 4141 0674 90

Accessory | Ordering No. | Remark
--- | --- | ---
Indexer | 4141 0150 95 |
HD indexer kit | 4141 0907 90 | Requires installing tool kit 4080 1120 80.

Accessory | Ordering No.
--- | ---
Indexing stop nut | 4141 0466 97
Countersink stop nut with scale | 4141 0843 91
Stop nut back | 4141 0823 93
Stop nut front | 4141 0841 91

Accessory | Ordering No. | Remark
--- | --- | ---
Conversion kit, right angle to in-line | 4141 0434 93 | Non-inboard lubrication tools
Conversion kit, in-line to right angle | 4141 0434 92 | Non-inboard lubrication tools