# Applications

The MWR-50 TA is a mechanical click-wrench combined with an electronic torque transducer.

The MWR-50 TA are equipped with the ISM band radio interface (characterized by a frequency equal to 868 MHz / 915 MHz) for wireless connection with Focus 61.

The MWR-50 TA works with Focus 61, which defines the tightening programs for the MWR-50 TA.

A | Focus 61 | B | Station 1
C | Station 2 | D | MWR-50 TA

For more information about the configuration and the use of the MWR-50 TA, refer to the Focus 61 User Guide.