# Product data

- Operating torque measuring range: 10 [N·m] - 50 [N·m] / 7.4 [lb·ft] - 36.9 [lb·ft]

- Drive: 9x12 mm.

- Overall length: 234 mm.

- Operating torque range: from 20% to 100% of the capacity

- Torque measurement accuracy (within the operating torque range): 2%

- Mechanical repeatability click: ± 4%

- Overload capacity: 120 % of nominal capacity

- Maximum angular speed: 250 °/s

- Angle measurement accuracy: ± 3.6 ° / 360 ° (at 6 ° per second)

- Temperature stability of torque measurement: +10 °C to +40 °C (10 °F to 104 °F)

- Tightening results memory capacity: 8100 Data sets (maximum)

- MWR-50 TA Reference Firmware version: 3.0.0

- Power supply: 1.2 V rechargeable battery