# Correct handling and click tightening

- The screw should be tightened in even strokes.

- The closing speed should allow an immediate interruption of the tightening operation as the MWR-50 TA clicks.

- The operation of the MWR-50 TA must be carried out by the middle of the handle.

- The force should be one-handed, uniform, parallel and applied with no interruptions until the tool clicks.

After the automatic release (click), the MWR-50 TA must not be moved further.