# MWR Charging cradle

To recharge the battery of the MWR-50 TA with the MWR Charging Cradle:

1. Connect the MWR Charging Cradle to the AC power.

2. Insert the MWR-50 TA into the MWR Charging Cradle:

   When the wrench is placed into the MWR Charging Cradle, the red, yellow and green LEDs (placed on three sides of the MWR-50 TA) flash alternately. This indicates that the wrench sets the internal offset (zero point) for the torque transducer and runs a quick self-test.

   When the MWR-50 TA is in charging mode and the internal offset has been performed, the yellow LED of the MWR-50 TA is on and the Status LED of the MWR Charging Cradle is flashing (green colored).

   When the charging process of the MWR-50 TA is complete, the Status LED of the MWR Charging Cradle is constantly on (green colored).

For more information on the MWR Charging Cradle functioning, refer to the MWR Charging Cradle Product Instructions.