# ETV STB34-30-10-BD

## Battery-Powered Nutrunner

# Product Information

# General Information

WARNING

Risk of Property Damage or Severe Injury

Ensure that you read, understand and follow all instructions before operating the tool. Failure to follow all the instructions may result in electric shock, fire, property damage and/or severe bodily injury.

- Read all Safety Information delivered together with the different parts of the system.

- Read all Product Instructions for installation, operation and maintenance of the different parts of the system.

- Read all locally legislated safety regulations regarding the system and parts thereof.

- Save all Safety Information and instructions for future reference.

In this Section

- Power Tool Information
- Safety Signal Words
- Warranty
- Website
- ServAid
- Safety Data Sheets MSDS/SDS
- Product Safety Video for Nutrunners
- Country of Origin
- Dimensional Drawings

# Power Tool Information

WARNING

Read all safety warnings, instructions, illustrations and specifications provided with this power tool.

Failure to follow all instructions listed below may result in electric shock, fire, and/or serious injury.

Save all warnings and instructions for future reference.

# Safety Signal Words

The safety signal words Danger, Warning, Caution, and Notice have the following meanings:

DANGER | DANGER indicates a hazardous situation which, if not avoided, will result in death or serious injury.
WARNING | WARNING indicates a hazardous situation which, if not avoided, could result in death or serious injury.
CAUTION | CAUTION, used with the safety alert symbol, indicates a hazardous situation which, if not avoided, could result in minor or moderate injury.
NOTICE | NOTICE is used to address practices not related to personal injury.

# Warranty

- Product warranty will expire in 12+1 months after dispatch from Atlas Copco's Distribution Center.

- Normal wear and tear on parts is not included within the warranty.

  - Normal wear and tear is that which requires a part change or other adjustment/overhaul during standard tool maintenance typical for that period (expressed in time, operation hours or otherwise).

- The product warranty relies on the correct use, maintenance, and repair of the tool and its component parts.

- Damage to parts that occurs as a result of inadequate maintenance or performed by parties other than Atlas Copco or their Certified Service Partners during the warranty period is not covered by the warranty.

- To avoid damage or destruction of tool parts, service the tool according to the recommended maintenance schedules and follow the correct instructions.

- Warranty repairs are performed only in Atlas Copco workshops or by Certified Service Partners.

Atlas Copco offers extended warranty and state-of-the-art preventive maintenance through its ToolCover contracts. For further information, contact your local Service representative.

For electrical motors:

- Warranty will apply, only when the electric motor has not been opened.

# Website

Information concerning our Products, Accessories, Spare Parts and Published Matters can be found on the Atlas Copco website.

Please visit: www.atlascopco.com.

# ServAid

ServAid is a portal that is continuously updated and contains Technical Information, such as:

- Regulatory and Safety Information

- Technical Data

- Installation, Operation and Service Instructions

- Spare Parts Lists

- Accessories

- Dimensional Drawings

Please visit: https://servaid.atlascopco.com.

For further Technical Information, please contact your local Atlas Copco representative.

# Safety Data Sheets MSDS/SDS

The Safety Data Sheets describe the chemical products sold by Atlas Copco.

Please consult the Atlas Copco website for more information www.atlascopco.com/sds.

# Product Safety Video for Nutrunners

Learn more about safety features on Atlas Copco nutrunners and what measures the operator has to take for a safe operation. Click the link or scan the QR code below to view the video:

https://www.youtube.com/watch?v=FAh6yttvUpw

# Country of Origin

For the Country of Origin, please refer to the information on the product label.

# Dimensional Drawings

Dimensional Drawings can be found either in the Dimensional Drawings Archive, or on ServAid.

Please visit: https://webbox.atlascopco.com/webbox/dimdrw or https://servaid.atlascopco.com.

# Overview

# Ambient Temperature

For best battery performance and life time, keep battery within temperature intervals.

Operating temperature, charge | +5 to +40 °C (+41 to +104 °F)
Operating temperature, discharge | 0 to +40 °C (+32 to +104 °F)
Transportation temperature | −20 to +40 °C (−4 to +104 °F)
Storage temperature | +10 to +25 °C (+50 to +77 °F)

Do not place battery in direct sunlight.

# Technical Product Data

Technical Product Data can be found on either ServAid, or the Atlas Copco website.

Please visit: https://servaid.atlascopco.com or www.atlascopco.com.

If the Technical Product Data is not available on either website, please contact the local Atlas Copco Customer Center for assistance.

# Installation

# Installation Requirements

# Installation

For installation guideline, see Power Focus 6000 user guide.

# Installation Instructions

# Wireless Communication

This tool supports both WLAN 2.4 and 5 GHz (except AdHoc), as well as Bluetooth.

The configuration of WLAN and Bluetooth is handled in Tools Talk Service 2.

# Attaching and Removing the Battery

1. Attach the battery to the tool and make sure that it is fastened correctly. The battery can be attached pointing forward or backward, to get the best accessibility and balance.

2. To remove the battery, press the button on the battery and push it out.

# Operation

# Ergonomic Guidelines

Consider your workstation as you read through this list of general ergonomic guidelines to identify areas for improvement in posture, component placement, or work environment.

- Take frequent breaks and change work positions frequently.

- Adapt the workstation area to your needs and the work task.

  - Adjust for a convenient reach range by determining where parts and tools need to be located to avoid static load.

  - Use workstation equipment such as tables and chairs appropriate for the work task.

- Avoid work positions above shoulder level or with static holding during assembly operations.

  - When working above shoulder level, reduce the load on the static muscles by lowering the weight of the tool, using for example torque arms, hose reels or weight balancers. You can also reduce the load on the static muscles by holding the tool close to the body.

  - Take frequent breaks.

  - Avoid extreme arm or wrist postures, particularly during operations requiring a degree of force.

- Adjust for a convenient field of vision that requires minimal eye and head movements.

- Use appropriate lighting for the work task.

- Select the appropriate tool for the work task.

- In noisy environments, use ear protection equipment.

- Use high-quality inserted tools and consumables to minimize exposure to excessive levels of vibration.

- Minimize exposure to reaction forces.

  - When cutting:

    A cut-off wheel can get stuck if the cut-off wheel is bent or not guided properly. Always use the correct flange for the cut-off wheel and avoid bending the cut-off wheel during operation.

  - When drilling:

    The drill might stall when the drill bit breaks through. Use support handles if the stall torque is high. The safety standard ISO11148 part 3 recommends using a device to absorb a reaction torque above 10 Nm for pistol grip tools and 4 Nm for straight tools.

  - When using direct-driven screwdrivers or nutrunners:

    Reaction forces depend on the tool settings and joint characteristics. Strength and posture determine the amount of reaction force that an operator can tolerate. Adapt the torque setting to the operator's strength and posture and use a torque arm or reaction bar if the torque is too high.

- In dusty environments, use a dust extraction system or wear a mouth protection mask.

# Operating Instructions

# LED Indicator (HMI)

LED Indicator | Description
--- | ---
Connection | Indicates the connection to the paired controller or software system.
Batch | Indicates when the batch is done.
Battery | Indicates battery status (flashing light = low battery, steady light = empty battery).
Alarm | A failure or event is detected.

# Tightening

WARNING

Risk of Injury

Make sure that the correct parameter file is being used. Wrong parameter file might cause too high torque with bodily injury as a result.

- Compare the maximum torque which is shown in the controller, with the maximum torque stated in the technical data of the tool, they should be the same.

## Rotation Direction for the Tightening

Check that the tool is in the correct running direction by turning the reverse button or reverse ring.

Pistol Grip Models (with side buttons)

- Press the reverse switch on the right hand side of the tool, to set the direction clockwise (CW).

- Press the reverse switch on the left hand side of the tool, to set the direction counter-clockwise (CCW).

Pistol Grip Models (without side buttons)

- Double press the function button on the top of the start trigger to shift the direction between clockwise (CW) and counter-clockwise (CCW).

Angle Models

- Turn the reverse ring to the right, to set the direction clockwise (CW).

- Turn the reverse ring to the left, to set the direction counter-clockwise (CCW).

## Soft Start

The soft start function facilitates the screw head and thread to reach the snug level. The duration of the soft start is adjustable.

For further information about tightening, see Power Focus 6000 Configuration manual.

# Scanner

WARNING

Laser Radiation

This device emits CDRH Class 2 and IEC 60825-1 Class 2 laser radiation.

WARNING

Laser Radiation

- Do not stare into beam.

# Lock-off Lever

The function of the lock-off lever is to avoid unintentional starting of the tool.

Flip the lock-off lever trigger to lock/unlock the safety function. Always put the lever in locked position before putting away the tool.

- Make sure the tool is equipped with a lock-off lever.

- Make sure that the lock-off lever works correctly.

- Replace the lock-off lever if it does not work correctly.

- Never remove the lock-off lever or lock it with tape.

Locked position.
Unlocked position.

# Dual Trigger

## Dual trigger (Recommended to use during operation)

WARNING

Crushing Hazard

The Dual trigger forces the user to use both hands to operate the tool. If not used, the operator can accidentally start the tool while adjusting the crowfoot, thus resulting in a serious hand injury.

- Make sure the tool cannot be started once the Dual trigger has been released.

- Always test the tool by first releasing the trigger of the Dual trigger, then push the trigger of the tool. If the tool starts; stop working.

# Service

# Preventing ESD Problems

The components inside the product and controller are sensitive to electrostatic discharge. To avoid future malfunction, make sure that service and maintenance is carried out in an ESD approved work environment. The figure below shows an example of an appropriate service work station.

# Maintenance Instructions

# Service Recommendations

Preventive maintenance is recommended at regular intervals. See the detailed information in Preventive Maintenance. If the product is not working properly, take it out of service and inspect it.

If no detailed information about preventive maintenance is included, follow these general guidelines:

- Clean appropriate parts accurately.

- Replace any defective or worn parts.

# Preventive Maintenance

# Maximizing Battery Life

Do not leave the battery connected to the tool if you do not use the tool for several days. The battery can discharge and go into “sleep mode” which will require a special wake-up charge procedure. For further information, see instructions for multicharger, 4211542485.

# Overhaul

Have your power tool serviced by a qualified repair person using only identical replacement parts. This will ensure that the safety of the power tool is maintained.

Service must only be carried out by qualified personnel who have access to the Service instruction and/or have been trained for service on this tool.

The electric motor is a sealed unit and may under no circumstances be opened by anyone else than Atlas Copco Industrial Technique AB.

If it is judged that the electric motor is defect or in need of service, the complete motor unit should be returned to Atlas Copco Industrial Technique AB for exchange.

Motors which have been opened by anyone else than Atlas Copco Industrial Technique AB will not be serviced.

Overhaul and preventive maintenance is recommended at regular intervals once per year or after maximum 250.000 tightening depending on which occurs sooner. More frequent overhaul may be needed if the machine is used in heavy-duty operations. If the machine not is working properly, it should immediately be taken away for inspection.

The backup battery must be replaced within 24 months from the tool's production date, or last battery backup replacement. Shorter interval if tool has been used in the higher accepted temperature range. A replaced backup battery should be recycled according to the Recycling Instruction. Spare backup batteries must not be stored in ambient temperatures above 300C and should due to self-discharge not be stored more than 6 months before powering it up for 4 hours. Spare backup batteries can be stored in a fridge (non-condensing environment).

When dismantling the tool always use the specially designed service tool 4080 0848 80, (two service tools are required).

# Lubrication Instructions

# Lubricant Guide

Part | Lubricant
--- | ---
Planetary gears with bearings | Molycote BR2 Plus
Angle gears with bearings | Atlas Gear Grease 270 (Tools configured with 110° angle head (-SZ), may also use Molycote Longterm 2 plus.)
Threads, O-rings, other | Almagard LE 3751

# Lubrication

Lubricate according to the Lubrication Guide at each service occasion.

For more information, see Spare Parts section in ServAid - https://servaid.atlascopco.com.

# Troubleshooting

# Overheated Tool

The tool can handle any normal line jobs that an operator sustains with the proper adjustments.

The tool temperature can be influenced by the following parameters:

- short cycle time

- torque above rated

- too low speed

- very high prevailing torque

- very soft joints

- ambient temperature

# Recycling

# Environmental Regulations

When a product has served its purpose, it must be recycled properly. Dismantle the product and recycle the components in accordance with local legislation.

Batteries may contain hazardous substances that can cause serious harm to the environment, human health, and safety if not handled correctly. Do not dispose of batteries in household waste. Batteries must be collected separately for recycling and must be placed in a battery recycling bin. This product and its information meet the requirements of the Battery Regulation (EU) 2023/1542 and must be handled in compliance with the regulation. Batteries are marked with a crossed-out wheeled bin symbol without a single black bar underneath. The battery must be recycled either according to local regulations or sent to your local Atlas Copco Customer Center for handling. Batteries must be handled by trained personnel only. By returning used batteries through proper collection channels, you help prevent environmental harm and enable the recovery of valuable raw materials.

# Recycling Instruction Scanner

Pos. | Part | Remarks | Recycle as
--- | --- | --- | ---
1 | Protective cover |  | Plastic, other, PU
2 | Scanner |  | Electronics

# Recycling Instruction

Pos. | Part | Remarks | Recycle as
--- | --- | --- | ---
a ETV has an Angle head. b ETC/ETO has an Angle head and an additional adapter and Closed end/Open end part. c ETD has no Angle head and instead a Front part.
1 | Angle headabc | This part can be different, depending on the model (ETV, ETC, ETO, ETD). The parts will all be recycled as the same material, as described in the table. | Metal
2 | Nut |  | Metal, Steel
3 | Planetary gear |  | Metal, Steel
4 | Nut |  | Metal, Steel
5 | Planetary gear |  | Metal, Steel
6 | Planetary gear |  | Metal, Steel
7 | Torque transducer |  | Electronic
8 | Motor |  | Electronic
9 | Nut |  | Metal, Steel
10 | Insulation hose |  | Plastic, Other, TPU
11 | Nut |  | Metal, Steel
12 | Com module |  | Electronic
13 | Led flex card complete |  | Electronic
14 | Reverse ring |  | Metal, Aluminum
15 | Electronics module |  | Electronic
16 | Handle body |  | Metal, Aluminum
17 | Trigger button |  | Metal, Steel
18 | Handle |  | Plastic, Other, PA
19 | Nut |  | Metal, Steel
20 | Nut |  | Metal, Steel
21 | Battery holder |  | Metal, Aluminum
22 | Electronics module |  | Electronic
23 | Battery (and back up battery for STB 34/64 |  | Battery, Li-lon
24 | Lid |  | Metal, Aluminum
25 | Backup battery |  | Battery, Li-lon
26 | Radio module |  | Electronic
27 | Lid |  | Plastic, Other, PA