# Installing Accessories

The disassemble of the tool or the accessories must only be performed by qualified maintenance personnel.

Make sure the battery is disconnected before starting to disassemble.

Required tools:

- Adjustable spanner

- Screwdriver

1. Loosen the front cap nut, using an adjustable spanner.

2. Remove the 4 screws fastening the two half-rings, behind the cap nut, and remove the two half-rings.

3. Connect the flex cable of the accessory, to the bus port marked 2.

4. Place the accessory, with the built in upper half ring, on the tool.

5. Fasten the accessory with the lower half ring, using the 4 screws included in the accessory box.

6. Tighten the front cap nut, using an adjustable spanner.