# Changing the Oil

For information about approved oils and grease see the Grease Guide.

1. Unscrew the two oil plugs on the side of the aluminum housing and drain the old oil.

2. Using a syringe, refill 12-14 ml of oil.

3. Clean the oil plug magnets.

4. Check the O-rings.

5. Screw the oil plugs back on the housing.

Service and lubrication of the planetary stage gearbox should be carried out by authorized personnel.

Relevant Information

- Grease Guide