# Práca s kartou Hlásenia

Tasks are configured in the Task menu. A task runs a tightening program and can be monitored from the Mobile GUI. The results of the task are presented in the Results menu.

To create a tightening program, create a task and select a strategy, either Tighten to Torque or Tighten to Torque plus Angle.

Programy na uťahovanie <meta-ref type="dynamic" name="AC.ITBA.RPD.name">Power Focus 6000 LV</meta-ref> potrebujú mať nastavené parametre, aby mohli uťahovanie vykonávať. Entering a value for Target Torque is mandatory, as well as Target Angle if Tighten to Torque plus Angle was chosen. Other settings are optional, such as Program name, Peak Torque and Angle. Proces uťahovania môžete monitorovať pridaním limitov, v rámci ktorých sa musí udržať uťahovací moment alebo uhol, v ktorom sa natáča matica.

It is possible to run two types of tightening programs from the Mobile GUI, Tighten to Torque and Tighten to Torque plus Angle.

Multistep programs and other types of tightening programs are available in the Web GUI, and should not be assigned to the Virtual Station 1, to avoid incorrectly displayed results.

V tejto sekcii

- Vytvorenie nového programu uťahovania
- Úprava programu uťahovania
- Odstránenie programu uťahovania