# 컨트롤러 탭 작업

Tasks are configured in the Task menu. A task runs a tightening program and can be monitored from the Mobile GUI. The results of the task are presented in the Results menu.

To create a tightening program, create a task and select a strategy, either Tighten to Torque or Tighten to Torque plus Angle.

<meta-ref type="dynamic" name="AC.ITBA.RPD.name">POWER FOCUS 6000</meta-ref> 조임 프로그램은 조임을 수행하기 위해 설정되어야 하는 매개변수가 필요합니다. Entering a value for Target Torque is mandatory, as well as Target Angle if Tighten to Torque plus Angle was chosen. Other settings are optional, such as Program name, Peak Torque and Angle. 또한 토크 또는 너트가 회전하는 각도를 유지해야 하는 한계를 추가하여 진행됨에 따라 조임을 모니터링할 수 있습니다.

It is possible to run two types of tightening programs from the Mobile GUI, Tighten to Torque and Tighten to Torque plus Angle.

Multistep programs and other types of tightening programs are available in the Web GUI, and should not be assigned to the Virtual Station 1, to avoid incorrectly displayed results.

이 섹션에서

- 조임 프로그램 생성
- 조임 프로그램 편집
- 조임 프로그램 삭제