# Utiliser l'onglet Coffret

Tasks are configured in the Task menu. A task runs a tightening program and can be monitored from the Mobile GUI. The results of the task are presented in the Results menu.

To create a tightening program, create a task and select a strategy, either Tighten to Torque or Tighten to Torque plus Angle.

Il est nécessaire de régler certains paramètres dans les programmes de serrage <meta-ref type="dynamic" name="AC.ITBA.RPD.name">Power Focus 6000 LV</meta-ref> pour permettre la réalisation d'un serrage. Entering a value for Target Torque is mandatory, as well as Target Angle if Tighten to Torque plus Angle was chosen. Other settings are optional, such as Program name, Peak Torque and Angle. Il est aussi possible de surveiller le serrage en cours en ajoutant des limites que doivent respecter le couple ou l'angle de rotation de l'écrou.

It is possible to run two types of tightening programs from the Mobile GUI, Tighten to Torque and Tighten to Torque plus Angle.

Multistep programs and other types of tightening programs are available in the Web GUI, and should not be assigned to the Virtual Station 1, to avoid incorrectly displayed results.

Dans cette section

- Créer un programme de serrage
- Modifier un programme de serrage
- Supprimer un programme de serrage