# Snabbstartguide

To provide a better overview of the system, the following instruction touches upon the steps that are required to start using the system.

The instruction does not cover all system features, but focuses on the most basic.

## Webb-GUI

1. Select the type of tool to use. The tightening strategies available, depend on the type of tool you select.

2. Detta görs genom att definiera ett åtdragningsprogram som innehåller alla relevanta parametrar för en åtdragning, till exempel målvinkel och målmoment. Huvudsyftet för verktyget är att utföra en åtdragning.

3. Skapa en Virtuell station och tilldela ett verktyg till den. Den virtuella stationen fungerar som ett gränssnitt mellan styrenheten och verktyget, vilket gör det möjligt att ansluta flera verktyg till en enda fysisk styrenhet. En virtuell station krävs även om endast ett verktyg är anslutet till styrenheten.

4. Tilldela en uppgift till den virtuell stationen. Uppgiften kan vara antingen ett åtdragningsprogram, en batchsekvens, eller en specificerad digital insignal (från exempelvis en streckkodsläsare). Verktyget som är tilldelat till stationen kan nu utföra uppgiften.

## Mobil GUI

1. Select the type of tool to use.

2. Create a tightening Task and set the relevant parameters, for example target torque and target angle. Huvudsyftet för verktyget är att utföra en åtdragning.

3. The created task will be assigned to a virtual station. Verktyget som är tilldelat till stationen kan nu utföra uppgiften.