# Fliken Arbeta med rapporter

Tasks are configured in the Task menu. A task runs a tightening program and can be monitored from the Mobile GUI. The results of the task are presented in the Results menu.

To create a tightening program, create a task and select a strategy, either Tighten to Torque or Tighten to Torque plus Angle.

I åtdragningsprogrammen för <meta-ref type="dynamic" name="AC.ITBA.RPD.name">POWER FOCUS 6000</meta-ref> behövs parametrar ställas in för att utföra åtdragning. Entering a value for Target Torque is mandatory, as well as Target Angle if Tighten to Torque plus Angle was chosen. Other settings are optional, such as Program name, Peak Torque and Angle. Det är även möjligt att övervaka åtdragningens förlopp genom att lägga till gränser, inom vilka momentet eller vinkeln som muttern vrids, ska hållas.

It is possible to run two types of tightening programs from the Mobile GUI, Tighten to Torque and Tighten to Torque plus Angle.

Multistep programs and other types of tightening programs are available in the Web GUI, and should not be assigned to the Virtual Station 1, to avoid incorrectly displayed results.

I detta avsnitt

- Skapa ett åtdragningsprogram
- Redigera ett åtdragningsprogram
- Ta bort ett åtdragningsprogram