# Trabajar con la pestaña Controlador

Tasks are configured in the Task menu. A task runs a tightening program and can be monitored from the Mobile GUI. The results of the task are presented in the Results menu.

To create a tightening program, create a task and select a strategy, either Tighten to Torque or Tighten to Torque plus Angle.

Los programas de apriete del <meta-ref type="dynamic" name="AC.ITBA.RPD.name">POWER FOCUS 6000</meta-ref> necesitan que se configuren los parámetros para realizar el apriete. Entering a value for Target Torque is mandatory, as well as Target Angle if Tighten to Torque plus Angle was chosen. Other settings are optional, such as Program name, Peak Torque and Angle. También es posible supervisar el apriete según progresa añadiendo límites dentro de los cuales se tiene que mantener el par o el ángulo en el que la tuerca gira.

It is possible to run two types of tightening programs from the Mobile GUI, Tighten to Torque and Tighten to Torque plus Angle.

Multistep programs and other types of tightening programs are available in the Web GUI, and should not be assigned to the Virtual Station 1, to avoid incorrectly displayed results.

En esta sección

- Crear un programa de apriete
- Editar un programa de apriete
- Borrar un programa de apriete