# Scanner and Tag for ETP SRB Tools

# Instruction Supplement

# General Information

The following scanners and tags are applicable:

2D Scanner ETP ST32 | 8433061555
AGILION ST TAG32 USD | 8433506410
ILT Tool Tag ETP | 8436677003
Scanner | 4220350790
Scanner | 4220504491
Selector | 4220350781
TLS ST TAG 32 U1 | 8433103010
TLS ST Tag 32 U2 | 8433203010
TLS ST TAG 32 USD2 | 8433505410
TLS ST TAG 32 USD1 | 8433504410
ILT Tag ETP 3in1 | 8436677013
ILM Tool Tag ETP | 8436677603
ILT Tool Tag ETP | 8436677003

# Intended Use

These scanners, tags and instructions only apply to ETP SRB tools.

# Mounting a Scanner or Tag to the Tool

When working on the assembly, use blunt plastic tweezers to avoid damaging parts or cables.
For torques and bolt sizes, refer to the applicable tool model in ServAid.

Steps 17 to 19 do not apply to ILM and ILT tool tags.

1. Remove the front part of the tool including the shaft.

2. Remove the four screws of the power module. Remove the power module.

3. Remove the five screws of the handle side cover. Remove the handle side cover.

4. Disconnect cables A and B from the handle module.

   A | Torque transducer
   B | Radio connector

5. Remove the screw of the ground plate top. Remove the ground plate top.

6. Remove the LED cover.

7. Remove the label plates and the lids on both sides of the tool.

8. Remove the cable cover.

9. Disconnect cables A-F from the handle module and cables G and H from the radio module.

   A | Speaker
   B | Tool board TBP
   C | HMI
   D | Light and conf.
   E | Motor temp.
   F | Commutation
   G | Antenna
   H | Antenna

10. Remove the screw from the main board module. Remove the main board module and the reverse button.

11. Pull the trigger and remove the pin by pulling it upwards.

12. Remove the trigger and the pin.

13. Separate the handle module from the motor module.

14. Remove the torque transducer.

15. Remove the LED flexcard.

16. Remove the two mounting screws of the accessory attachment.

17. Remove the four screws of the accessory lid. Remove the lid.

18. Pull the accessory cable through the accessory lid and connect the cable to the accessory circuit board if applicable.

19. Put the accessory lid back in place and tighten the four screws.

20. Pull the accessory cable through the hole of the new cable cover and insert it in place while pulling the cable.

21. Position the accessory in place and tighten the two screws of the accessory attachment.

22. Pull the cable under the motor module cover.

23. Reattach the LED flexcard.

24. Reattach the torque transducer.

25. Reinsert the label plates on both sides of the tool.

26. Reattach the LED cover.

27. Reattach the motor module to the handle module.

28. Put the front light back in place.

29. Insert the pin into the trigger and put the trigger back in place.

30. Pull the trigger and pull the pin downwards.

31. Put the main board module back in place and tighten the screw.

32. Put the reverse button back in place.

33. Reconnect cables A-F to the handle module and cables G and H to the radio module.

    A | Speaker
    B | Tool board TBP
    C | HMI
    D | Light and conf.
    E | Motor temp.
    F | Commutation
    G | Antenna
    H | Antenna

34. Put the ground plate top back in place and tighten the screw.

35. Connect cables A-C to the handle module over the ground plate top.

    A | Torque transducer
    B | AUX
    C | Radio connector

36. Put the handle side cover back in place and tighten the five screws.

37. Insert the shaft and fasten the front cover.

38. Put the power module back in place and tighten the four screws.

## Applies to:

4220 3507 81
4220 3507 90
4220 5044 91
8433 0615 55
8433 1030 10
8433 2030 10
8433 5044 10
8433 5054 10
8433 5064 10
8436 6770 03
8436 6770 03
8436 6770 13
8436 6776 03
8436 6776 11
8436 6776 13