# Emptying and Cleaning the Collection Containers

Screw abrasion collects in the Collection Containers. They must be emptied regularly, depending on the wear of the screws.

One Collection Container is located at the front, under the Feeding Tube Connection, and one on the back (lower illustration). The Collection Containers can be removed with a hex key after unscrewing the M5x8 screws and can then be emptied.

## Applies to: