# Packaging

The packaging is intended to protect the individual components from transport damage, corrosion and other damage during transport until assembly. The packaging must not be damaged under any circumstances and should only be removed immediately before assembly.

- The Screw Feeding Unit and the boxes are stacked on a pallet and wrapped in a film.

- The Screw Feeding Tightening Module is packed in a box with the accessories.

- The Power Focus 6000 is packed in a box.

## Applies to: