# Transporting the Screw Feeding Unit

WARNING

Crushing Hazard

Never place the Screw Feeding Unit on an unsecured surface. Due to vibrations, the Screw Feeding Unit can move on the surface it is placed on and fall, thus resulting in serious bodily injury.

- Secure the Screw Feeding Unit from falling.

- Place the Screw Feeding Unit where there is a stop edge or a surface with a suitable recess.

WARNING

Crushing Hazard

Never transport or carry the Screw Feeding Unit unassisted. The Screw Feeding Unit is heavy and if dropped, it can result in serious bodily injury.

- The Screw Feeding Unit may only be transported with the aid of suitable hoists with optional suspension.

- Two people must carry the Screw Feeding Unit using the handles.

- The Screw Feeding Unit is equipped with recessed grips on the left and right hand sides. For a short transport, these can be used to carry the unit. Optionally, a suspension can be mounted on the mounting plate (green).

- All connections should be removed before transport to avoid damage of the connecting cables.

## Applies to: