# Controls

No. | Description | Function
1 | Rotary Switch | Bit Change position: The Bit Complete on the Screw Feeding Tightening Module moves forwards, and the screw is ejected. Automatic position: The Bit Complete on the Screw Feeding Tightening Module moves backward, and a screw is loaded. Disabled for fixture feeders for uninterrupted automatic mode. Function can be enabled in feeders web HMI.
2 | Illuminated Push Button | Lit up in yellow in the event of an error. Errors can be acknowledged.
3 | Status Light | Lit up in white when ready. Unlit when switched off.
4 | Regulator | The compressed air supply.
5 | Shut-off Valve | Switch ON/OFF the compressed air supply and vent.

## Applies to: