# Bit Change Mode

1. Set the Rotary Switch in the "Bit Change" position.

2. The screw is ejected at the Feeding Head of the Screw Feeding Tightening Module and the Bit Complete moves forward.

   Now, for example, the Bit on the Screw Feeding Tightening Module can be changed.

3. After completing the change, set the Rotary Switch in the "Automatic" position.

   The Bit Complete in the Screw Feeding Tightening Module moves backwards and a screw is loaded.

Disable fixture feeders for an uninterrupted automatic mode. The function can be enabled in feeder’s web HMI.

## Applies to: