# Connecting the Screw Feeding Unit to the Compressed Air Supply

WARNING

Compressed Air

High air pressure can cause severe damage and bodily injury.

- Do not exceed maximum air pressure.

- Make sure that there are no damaged or loose hoses or fittings.

The compressed air must be free of any kind of contamination.

1. Use the Shut-off Valve (1) to switch off the compressed air supply. This will vent and secure against unwanted movement.

2. Connect the Tube for the compressed air supply to the Air Supply on the Screw Feeding Unit (2).

3. If all components of the Screw Feeding system are pneumatically connected, the compressed air supply can be reactivated by turning on the Shut-off Valve .

## Applies to: