# Replacing the Feeding Tube

WARNING

Risk of severe injury

Air under pressure can cause injury.

- Always shut off the air supply when not in use or before any adjustments.

- Drain the hose of air pressure and disconnect the tool from air supply when not in use or before any adjustments.

- Always use the correct hose size and air pressure for the tool.

1. Open the Cover Lid.

2. Unscrew the Clamping screw on the connection and pull off the Feeding Tube and the Feeding Tube Connection.

3. Push the new Feeding Tube onto the Feeding Tube Connection. Push the Feeding Tube Connection with the tube into the connection on the Screw Feeding Unit, then tighten the Clamping screw.

## Applies to: