# Feeding Tube

WARNING

High Air Pressure and Projectile Hazard

Always verify that all connections between the Feeding Tube and the Swivel Arm are securely fastened before pressurizing the tool. Otherwise screws can escape at high speed and cause serious injury, especially to the eyes.

- For this reason, the pneumatic power supply must be switched off and vented during all work on the Screw Feeding Tightening Module, or the "Bit Change" mode must be set on the Screw Feeding Unit.

The Feeding Tube transports the screws from the Screw Feeding Unit to the Swivel Arm of the Screw Feeding Tightening Module by air pressure.

No. | Description | Function
1 | Ring Sensor | Detects when the fastener leaves the seperation unit.
2 | Feeding Tube | Feeds the screws from the Screw Feeding Unit to the Screw Feeding Tightening Module
3 | Screw Feeding Tightening Module | Shows the setup with a Handheld Tightening Module. For further information about the other tightening modules, refer to the corresponding product information.

## Applies to: