# Insulated Cover ETV STR 30FS

## Attachments

# Declarations

# Regional Requirements

WARNING

This product can expose you to chemicals including lead, which is known to the State of California to cause cancer and birth defects or other reproductive harm. For more information go to

https://www.p65warnings.ca.gov/

# Safety

DO NOT DISCARD - GIVE TO USER

WARNING

Read all safety warnings, instructions, illustrations and specifications provided with this product.

Failure to follow all instructions listed below may result in electric shock, fire, property damage and/or serious injury.

Save all warnings and instructions for future reference.

WARNING

All locally legislated safety rules regarding installation, operation and maintenance shall be respected at all times.

## Statement of Use

- For professional use only.

- This product and its accessories must not be modified in any way.

- Do not use this product if it has been damaged.

- If the product data or hazard warning signs on the product cease to be legible or become detached, replace without delay.

- The product must only be installed, operated and serviced by qualified personnel in an industrial environment.

In this Section

- Intended use
- Product Specific Instructions

# Intended use

This product is intended for use on or in close proximity to energized electrical apparatus or conductors operating at maximum voltage of 1000 V.

# Product Specific Instructions

# General Installation Safety

WARNING

High Voltage Hazard

Insulated tool covers must always be used together with isolated sockets.

- Do not use insulated tool covers without isolated sockets.

- Install the insulated tool covers securely, always follow the installation instructions.

- Replace the insulated tool covers if they are damaged in any way.

In this Section

- Installation Overview

# Installation Overview

Legend to page 2.

To install the insulated tool cover, do the following:

1. Remove the front nut and the rubber ring from the insulated tool cover.

2. Separate the insulated tool cover in its two halves.

3. Attach the two halves of the insulated tool cover to the tool.

4. Fasten the front nut and attach the rubber ring in place onto the tool.

To remove the insulated tool cover, do the following:

1. Remove the front nut and the rubber ring of the insulated tool cover from the tool.

2. Remove the two halves of the insulated tool cover from the tool.

# General Operation Safety

WARNING

High Voltage Hazard

Accidental contact with any high voltage may result in severe injury or death.

- Always use insulated tool covers together with isolated sockets.

- Do not use insulated tool covers if they are damaged in any way or if they are not correctly installed.

- Only the parts of the tool covered by insulated tool covers are protected against high voltage. The other parts of the tool are not protected against high voltage.

## Inspection Before Use

- Visually inspect this product every time before use.

- If there is any doubt concerning the safety of this product, a suitably trained person must examine it and retest it, if necessary.

## Temperature

- Use this product in an industrial environment with a regulated temperature.

- Do not use this product in temperatures above 40°C or in high atmospheric humidity.

# General Service and Maintenance Safety

## Storage

- Store this product properly so as to minimize the risk of damage to the insulation due to storage or transportation.

- Store this product separated from other tools to avoid mechanical damage or confusion.

- Protect this product from excessive heat as well as from UV radiation.

## Periodic Examination

A suitably trained person should perform an annual visual examination of this product to determine its suitability for further service.