# Troubleshooting Symptoms and Required Action

Symptom | Probable Cause | Required Action
--- | --- | ---
Motor doesn’t run | 1.Check fuse 16 a Part# 10064 | 1. Change fuse 16 a (white - on top)
2. Check electrical box | 2. Check for disconnection
3. Check 115v cord | 3.Check for wire cut or disconnect
4. Check plug | 4. Check for wire disconnect
5.Check remote control | 5. Check for wire disconnect
Motor start difficult | 1. Bearing Part#10198 & 10178 | IA. Remove the pump from the tank IB. Remove block pump IC. Disassemble block pump ID. Change bearing
2. Remote control handswitch small white plastic support | 2A. Open the handswitch 2B. Replace small plastic parts
Blown fuses when starting | Check if fuse 16 a is blown Part# 10064 | To avoid the problem don’t run motor If hydraulic hose are not connected
Hose or tool fitting is damaged or leaks. | 1. Broken or melted plastic outer covering. | 1. If underlying plastic is still intact continue operation. Inspect frequently.If underlying plastic is still intact continue operation. Inspect frequently.
2. Frayed plastic strands. | 2. Cut hose in half and discard. Replace hose.
3. Oil leaks through fibres. | 3. Cut hose in half and discard. Replace hose.
4. Broken fittings. | 4. Remove old fitting and replace with STEEL high pressure fittings only. After changing fittings, always run test #5 to insure proper plumbing.
Electric pump will not run | 1. Loose electric connections in control box. | 1. Open control box and visually inspect for loose threaded or push-on connectors.
2. Motor burned up. | 2. Replace motor components whichever is necessary. SHOP JOB.
Fuse | 3. Change defect fuse