# Electric Connections

Ensure proper power availability to prevent motor failure or dangerous electrical overloading. Use the recommended amperage listed on the motor nameplate. Do not use electric pump if ground is not connected on plug.

尽量缩短延长线的长度，确保电线具有适当的线径并接地。

Extension cord should be #10 AWG gauge.

警告

Electric motors may spark. 不要在爆炸性环境中或存在导电液体的环境中使用电动泵。 Air driven pumps are better suited for these applications.