# Electric Connections

Ensure proper power availability to prevent motor failure or dangerous electrical overloading. Use the recommended amperage listed on the motor nameplate. Do not use electric pump if ground is not connected on plug.

연장 전선의 길이를 최소화하고 선 크기가 적절한지 그리고 접지되어 있는지 확인해 주세요.

Extension cord should be #10 AWG gauge.

경고

Electric motors may spark. Do not operate in an explosive atmosphere of in the presence of conductive liquids. Air driven pumps are better suited for these applications.