# Electric Connections

Ensure proper power availability to prevent motor failure or dangerous electrical overloading. Use the recommended amperage listed on the motor nameplate. Do not use electric pump if ground is not connected on plug.

Reduza o comprimento das extensões e confirme se a bitola do fio e o aterramento são adequados.

Extension cord should be #10 AWG gauge.

AVISO

Electric motors may spark. Do not operate in an explosive atmosphere of in the presence of conductive liquids. Air driven pumps are better suited for these applications.