# Lubrication

To keep the wrenches in good working condition, lubricate the drive components periodically between service intervals.

Disassembly before lubrication:

1. Remove the sideplate screws and sideplate [1].

2. Remove the drive assembly [2].

Do the following actions during lubrication maintenance:

1. Examine the drive pin and springs for signs of wear or damage. Replace the drive pin and springs if necessary.

2. Examine the edges of ratchet teeth for signs of damage. Replace the ratchet if necessary.

3. Examine the drive pawl teeth for signs of damage. Replace the drive pawl if necessary.

4. Examine the drive pawl springs for signs of damage. Replace the springs if necessary.

5. Lubricate the shaded areas with Molykote 1000.

The procedure for assembly is the same as for disassembly but backwards.