# Basic Tool Operation

- Wear PPE – Correct & appropriate safety equipment must be worn.

- Connect hoses - Ensure all hose connections are secure and correctly made. Confirm hoses are free from defects.

- Cycle the tool – Place the tool on a flat surface, turn pump on. Press the ADV button on the pump remote until tool clicks. Release, wait for tool to click. Repeat.

- Set pressure – Press the ADV button and slowly turn the pressure regulator clockwise to reach the correct pressure.

## For optimum performance:

Frequently inspect tool, power pack, hoses, connectors, electric cables and accessories for visual damage. Always follow instructions for tool and pump maintenance.

## For optimum safety:

Always perform a task based risk assessment prior to tool/system use.