# Installation Safety

A | WARNING Should a gap appear during use stop operation immediately.
B | WARNING Pinch point hazard, do not place hands in this area.
C | WARNING Never handle pressurise hoses. Oil escaping under pressure could impregnate skin.

## Ensure nut of corresponds with tool of size and always ensure a solid reaction is available.

## Never Kink or bend hoses excessively.

## Never strike wrench to assist breakout.