# Seal Replacement

1. This section details the replacement of “Clip - In” type high pressure seals.

2. Insert the inner seal into the seal housing; the seal clip fits into the seal clip housing.

3. Using a blunt nose tool push the seal fully into the seal clip housing, work around the periphery of the seal until the seal is completely inserted into the clip housing.

4. Insert the outer seal into the seal housing; the seal clip fits into the seal clip housing.

5. Using a blunt nose tool push the seal fully into the seal clip housing, work around the periphery of the seal until the seal is completely inserted into the clip housing.

## Applies to: