# Tensioner Arrangement – 50% Configuration

Every other bolt simultaneously tensioned.

Every other bolt consists of adequate bolt protrusion.

In this configuration the bolt to tensioner ratio is 50%. The tensioning procedure consists of:

- Simultaneously tensioning every other bolt, to first pass pressure “A”

- Tension the final 50% of the bolts, to 2nd pass pressure “B”

- Optional checking pass.

WARNING

Projectile Hazard

Never pressurize an unconnected male coupler. Male couplers are not designed to withstand high pressure, in the unconnected mode. Pressurizing an unconnected male coupler can lead to serious bodily injury or death.

- If you are left with an unconnected male connection, check the hydraulic hose assembly and correct the error.

## Applies to: