# Tensioning procedure 100% bolt to tensioner ratio configuration

1. Ensure the two halves of the bolted joint are full aligned.

2. Fit the tensioners to all of the bolts See also Tensioner System Configuration or illustrations of tensioner set up and Tensioner Installation for installation instructions.

3. Using link hoses connect the tensioners together and to a suitable pump unit. See also Tensioner System Configuration for configuration illustrations and for link hose connection instructions. Before connecting a link hose to the pump unit make sure the pump is turned off and the pressure release valve is in the open position.

4. Ensure the tensioning team is aware of the target working pressure. Only qualified engineers who have been appropriately trained or have suitable experience in bolting technology should perform bolting calculations.

5. For pump operation refer to the supplied pump instruction document. Operate the pump unit and pressurize the system to 1000psi (70 bar) and check that the pressure is holding steady. If the pressure drops investigate the problem looking for leaks.

6. Once the pressure is holding steady, continue to pressurize the system up to the target calculated working pressure. Continually monitor for piston over stroke, should any piston over stroke indicator become visible immediately stop the pump to hold the pressure, go to step 8 then 9 then 10. Then recommence the tensioning procedure from step 5.

7. Once the target working pressure is reached, stop the pump to hold pressure. Monitor the pump pressure gauge to ensure the pressure is neither falling nor rising.

8. Once the pressures is holding steady approach the tensioners and by using a tommy bar inserted into the nut socket holes rotate the nuts firmly against the joint face. Repeat until all of the nuts have been firmly seated against the bolted joint.

9. Slowly open the pressure relief valve, the pressure will drop to zero.

10. (OPTIONAL) If the pistons are close to their fully extended position, use a tommy bar inserted into the thread inserts and wind down the inserts to close the pistons to their zero stroke position.

11. Repeat steps 5 through 10 for a second time.

12. Repeat steps 5 through 10 for a third time.

13. Using a tommy bar inserted into the holes in the thread insert head, rotate the thread insert to close the tensioner piston to zero. Repeat until the pistons are fully closed.

14. Dis-connect all hydraulic hoses and remove all tensioners from the bolted joint. The tensioning procedure is considered complete.

## Checking Procedure

Pressurize the system for a 4th time and try to seat the hexagon nuts. Use a tommy bar inserted into the nut sockets try to tighten down the nuts further by hand.

- If there is no further rotation of the nuts, the tensioning sequence is considered complete. Slowly open the pressure relief valve, the pressure will drop to zero. Continue from step 14.

- If further nut rotation is achieved, repeat steps 6 through 11 until no further nut rotation is possible.

## Applies to: