# Hydraulic Fluid

The performance of hydraulic equipment is heavily dependent on the quality and characteristics of the hydraulic fluid selected for use. The choice of the specification and viscosity of the hydraulic fluid should be based of the conditions of use, taking into account several factors as follows:

- The range of environmental temperature.

- The range of oil viscosity defined for the equipment.

- The application (range of pressures, sources of contamination of the hydraulic fluid, the type of pump, etc.)

- The ease of getting a proper replacement or equivalent hydraulic fluid.

  Example: ISO Grade 15, 32 and 68.

  For changing or refilling the oil, it is recommended to use the same oil as supplied with the pump.

## Hydraulic Oil Selection Chart

Please use the link below to find our safe data sheets for Maximizer.

https://www.atlascopco.com/en-uk/sys/safetydatasheets