# Pump Preparation

1. Ensure the pressure release valve is in the open position (rotate anti-clockwise to stop). The pressure relief valve is fitted with a torque limiter to prevent over tightening it. Limiter will ‘Click Out’ as a preventative measure.

2. Ensure the On/Off valve is in the off position.

3. Connect the air hose to the air inlet connector. Give the hose a sharp tug afterwards, to ensure a solid connection.

4. Connect the hydraulic link hose to the female quick connector. (Refer to the operation manual supplied with your tensioners for correct hydraulic link hose configuration)

5. Ensure an adequate volume of oil is contained in the Oil Tank.