# Before Initial Operation

- Carry out a visual inspection before each start-up.

- Check remote control, mains plug and all cables for damage.

- Check hose couplings, hoses and hydraulic torque tools for damage.

Hoses and hydraulic torque tools are not included in delivery.

- Hose couplings, hoses and hydraulic torque tools must be designed for an operating pressure of Max.700 bar / 10,000 PSI..

- Hose couplings, hoses and hydraulic torque tools with lower operating pressures are not permitted to be connected to the pump unit.

- Check the entire machine, fluid reservoir, motor, manometer and air line lubricator for damage such as ruptures or leaks.

- Have damaged parts replaced by qualified technicians before operation.

- Check hose couplings for dirt.

- Clean soiled hose couplings before operation.

- Check the fluid level; the level must be up to the middle of the oil sight glass; top up hydraulic fluid, if needed. Use recommended grade of oil as per chart see also,Hydraulic Fluid

- Set up the pump unit on a level, horizontal surface so that it is prevented from falling over or falling down.

- Connect the pump unit by means of the threaded couplings with the hoses and with the hydraulic torque tool.

  Refer below picture to check section,

- Connect the pump unit to the air supply.

- Ensure a dynamic pressure of 5-6 bar and air volume of minimum 40 cfm is available. Higher pressures can lead to excessive wear and tear or damage the seals / valves.

The pump unit must not be operated without the hoses and the hydraulic torque tool connected up.