# General Instructions

The tool may only be used together with the associated torque reaction bar, which is adapted to the screw joint application concerned.

1. Attach the reaction bar to the tool and insert the retaining ring into the groove to hold the reaction bar in position.

2. Attach the socket to the square drive. Insert the locking pin through the socket and square drive according to the illustration.

WARNING

Crushing Hazard

Check the rotational direction of the tool before start! A start in an unexpected rotational direction can cause bodily injury or property damage. Moving parts can crush and cut.

- Make sure that the rotational direction of the tool is correct before starting the tool.

- Keep hands and fingers away from moving parts.