# Error Codes

Error format: E<Error Group>-<ErrorCode>

Error code is for internal use only.

If the error is not solved, contact Atlas Copco representative.

Error Group
Error Category
Service Hints
Search

Error Group | Error Category | Service Hints
--- | --- | ---
none | item | none
00 | Error updating tool SW | SW update issue. Try to connect tool to TTS2. It may give more info.
01 | General SW error | General software issue. Update to latest software.
02 | General SW error | General software issue. Update to latest software.
03 | Front light error | Front light issue. Check cable and/or replace board.
04 | Tool HMI error | Tool HMI error. 1. Update software using FFU flag. 2. Check cable.
05 | General SW error | Motor control issue. 1. Check Main board (MB) - Motor control board (MCB) connection. 2. Update to latest software.
06 | Tool memory error | Parameter memory issue. Try connecting tool to TTS2 to reset factory parameters.
07 | Motortune error | Motor tune issue. 1. Update software to latest. 2. Try running tests in TTS2. 3. Check that the commutation board in the back of the tool is mounted correctly. A possible problem is that it isn't pushed properly into place.
08 | General SW error | Parameter issue. Try connecting tool to TTS2 to reset factory parameters.
09 | General SW error | Radio issue. 1. Check cable. 2. Check tool antennae cable. 3. Update software with FFU-flag.
10 | Error updating radio SW | Radio SW update issue. 1. Check cable. 2. Check tool antennae cable. 3. Update software with FFU-flag.
11 | General SW error | Radio issue. 1. Check cable. 2. Check tool antennae cable. 3. Update software with FFU-flag.
12 | General SW error | Radio Bluetooth issue. 1. Check cable to radio module. 2. Update software with FFU-flag.
13 | General SW error | Radio WIFI issue. 1. Check cable for radio module. 2. Update software with FFU-flag.
14 | General SW error | Smart web-configuration issue. 1. Check cable for radio module. 2. Update software with FFU-flag.
15 | RBU HW error | IAM issue. Try resetting SD-card checksums in TTS2.
16 | RBU HW error | IAM issue. Try resetting SD-card checksums in TTS2.
17 | General SW error | Parameter memory issue. Try connecting tool to TTS2 to reset factory parameters.
18 | General HW error | Indicator board issue.
19 | General SW error | General software issue. Update to latest software.
20 | General SW error | Internal communication issue. Check Main board - Motor control board connection.
21 | General SW error | Internal communication issue. Check Main board - Motor control board connection.
22 | General SW error | General software issue. Update to latest software.
23 | Backup battery error | Backup battery issue. Check backup battery connection.
24 | General SW error | General software issue. Update to latest software.
25 | Error updating motor control board | Motor control board (MCB) software update issue. 1. Check MCB connection. 2. Update to latest software.
26 | General SW error | Motor control board communication error. 1. Check MCB connection. 2. Update to latest software.
27 | General SW error | General hardware or software issue.
28 | Power supply error | General power supply issue.
29 | General SW error | Tool device identification issue. Connect to TTS2, may help to re-write tool identity.
30 | General SW error | Tool device identification issue. Connect to TTS2, may help to re-write tool identity.
31 | General SW error | Torque transducer issue. Check torque transducer and cable.
32 | General tightening error | General tightening error.
33 | Tool trigger error | Tool trigger issue. 1. Test trigger in TTS2. 2. Check that trigger is not broken. 3. Replace main board.
34 | General SW error | Tightening trace issue.
35 | General SW error | Tightening trace issue.
36 | General HW error | Problem with hardware or connection between MB/MCB boards. 1. Check mechanical connection. 2. Replace MCB and/or MCB.
37 | Function button error | Problem with changing tool direction. 1. Test function button in TTS2. 2. Update SW to latest version.
38 | General HW error | Torque transducer issue. Check torque transducer and cable.
39 | General HW error | General HW issue.
40 | General HW error | General HW issue. Try replacing MB.
41 | Error updating tool SW | SW update issue. Try to connect tool to TTS2, it may give more info.
42 | Error updating tool SW | SW update issue. Try to connect tool to TTS2, it may give more info.
43 | General HW error | Indicator board issue. <SRB HA does not use the indicator board>
44 | General HW error | Second trigger issue. 1. Check cable and second trigger board. 2. Disconnect Gear ID board from front light board. 3. Replace front light board.
45 | Error reading SRB HA tool config | Parameter memory issue. Try connecting tool to TTS2 to reset factory parameters.
46 | General SW error | SRB HA - Smart result issue. 1. Try removing "RESULT.CSV" from IAM in folder HA. 2. Update software.
47 | General SW error | SRB HA - Smart program issue. 1. Update to latest tool software. 2. Restore factory settings in TTS2.
48 | General SW error | SRB HA - Smart program or Set&Go issue. 1. Update to latest tool software. 2. Restore factory settings in TTS2.
49 | General SW error | General software issue. Update to latest software.
50 | General HW error | IAM SD-card issue.
51 | General SW error | General software issue. Update to latest software.
52 | General SW error | Parameter memory issue. Try connecting tool to TTS2 to reset factory parameters.
53 | Open end configuration error | Open end configuration issue. <SRB HA does not support this feature>
54 | General SW error | General HW issue.
55 | Front light HW error | Front light issue. 1. Check cable and/or replace board. 2. Update to latest software.
56 | Push button error | Function button error. Runt function button test in TTS2. Replace button board or cable.
57 | General SW error | HW input error. Try replacing Main board.
58 | General SW error | HW input error. Try replacing Main board.
59 | General SW error | Problems settings up Radio module in Access point mode.
60 | Error updating indicator board SW | Indicator board issue. <SRB HA does not use the indicator board>
61 | General SW error | Front light communication issue. Check cable and front light board.
62 | RBU HW error | IAM SD-card issue.
63 | General HW error | Main board FPGA error. 1. Try updating with latest software. 2. Replace main board.
64 | General HW error | Main board FPGA update issue. 1. Try updating with latest software with FFU flag. 2. Replace main board.
65 | General HW error | Parameter memory issue. Try connecting tool to TTS2 to reset factory parameters.
66 | General SW error | Internal communication issue. Related to Radio or TTS2 communication.
67 | General SW error | Internal communication issue. Related to Radio or TTS2 communication.
68 | General SW error | Internal communication issue. Related to Radio or TTS2 communication.
69 | General SW error | General SW issue.
70 | General SW error | General SW/HW issue.
71 | General SW error | General SW/HW issue.
72 | General SW error | General SW issue.
73 | Software update error | General SW update issue.
74 | FH_ECG_ToolsTalkServices2Test | Issue with TTS2 enabled tests.