# Assembling HD indexer kit

WARNING

Make sure that the air supply is not connected.

CAUTION

Wear gloves to avoid personal injury because of sharp cutting edges. Only experienced maintenance personnel can assemble or disassemble the product.

Required tools

- Open-end spanner

- Indexer installing tool kit

1. Position the indexer housing onto the block.

2. Put the nut into the indexer housing, with the threads downwards. Tighten the nut with the indexer installing tool.

3. Put the waved washer and the shaft. With the splines downwards, into the indexer housing.

4. Push the button on the indexer housing, so the nut easily moves down to the bottom. Tighten the front nut on the shaft onto the indexer housing with an open-end spanner.