# Installing the indexer

WARNING

Make sure that the air supply is not connected.

CAUTION

Wear gloves to avoid personal injury because of sharp cutting edges. Only experienced maintenance personnel can assemble or disassemble the product.

Required tools

- Allen key

Make sure the following components are removed from the drill:

- Spindle cover

- Front part

- Drill bit

1. Remove the connector using an Allen key.

2. Replace the connector with the indexer and put it in position. Tighten the index with an Allen key.

Put the above components back after finishing the installation.