# Operating the drill

To start drilling... | push the start button.
To stop drilling and retract the spindle into the start position... | push the retract button.
To switch off the motor in case of emergency... | push the emergency stop button.
To reset the emergency stop and restore normal operation... | disconnect the air hose. Pull the emergency stop button, reconnect the air hose to reset the air logic.